Title: GB_parts.xlsx
Author: JimZ

PARTS LIST KIT N0. 0851 ‐ Cloud Hopper
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | PAPER BODY TUBE | BT‐5BJ | 30304 | 2" long | 0.515" ID | 0.541" OD | 0.013" wall | Glassine
1 | ENGINE HOLDER | EH‐3 | 3143 | 1.8" long | .125" wide | .025" thick | | Mini
1 | PAPER ADAPTER | RA‐560 | 30120 | .542" ID | 1.594" OD | .05" thick | One ring notched. | Set of 2
1 | PAPER BODY TUBE | BT‐60R | 30418 | 5" long | 1.595" ID | 1.637" OD | 0.021" wall | Glassine
1 | BALSA FIN STOCK | *BFS‐30(4x9) | N/A | 4" wide | 9" long | 3/32" thick | 0.09375 | Scan
1 | LAUNCH LUG | LL‐2A | 38175 | 5/32" ID | 1/8" rod | 1.25" long | | Mylar
1 | Shock Cord Mount | SCM‐50 | 84444 | 1.5" wide | 3" long | 67 lb. Cardstock | BT‐50 & larger | Scan
1 | Shock Cord | SC‐1B | 85734 | 1/8" wide | 12" long | | | Rubber
1 | PLASTIC NOSE CONE | *PNC‐60L | 71019 | 2.5" long | 1.637" OD | 1.58" ID | 0.25" ridge | Injection Molded 1 of 2
1 | NOSE CONE ADAPTER | *PNCA‐60L | 30103 | 1" long | 1.57" OD insert | .75" shoulder | .25" insert | Injection Molded 2 of 2
1 | Parachute | PK‐12 | 82054 | 12" dia. | 1.25 mil thick | LDPE plastic | Org/Wht | Damon Logo
1 | Shroud Line | SLT‐72 | 38237 | 72" | .020" diameter | Twisted cotton | 3 x 24" shrouds |
1 | Tape Disc | TD‐3F | 38406 | 1/2" dia. | Paper | Self‐Stick | WO/Center Hole | Set of 6
1 | Display Stand | SP‐MBDS | 9014 | 8.5" long | 5"wide | Blk, Blu | 110 lb. Cardstock | Scan
1 | Dummy Engine Casing ‐ | EC‐8 | 35014 | 0.5" OD | 1.75" long | Empty Casing | |
1 | Decal Sheet | KDS‐0851 | 37351 | 4" wide | 5" long | Red, Yel | Selfstick | Scan & Redraw
*Die‐Cut Fin Sheet is BF‐00851.
*PNC‐60MS is the blow molded replacment and can be used to substute the PNC‐60L and PNCA‐60L combination.