Title: est2114_parts.xlsx
Author: JimZ

PARTS LIST KIT N0. 2114 ‐ Corkscrew
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | Nose Cone/Tube Coupler | NC‐1090 | 72630 | OD 1.090" | 3.5" Long | W/Coupler | White | Blow Molded
1 | PAPER BODY TUBE | HBT‐1090 | 031212 | 4.75” long | 1.090" OD | 1.030" ID | 0.030" wall | White
1 | PAPER BODY TUBE | HBT‐1090 | 85878 | 11" long | 1.090" OD | 1.030" ID | 0.030" wall | White slotted for 3 fins
1 | PAPER BODY TUBE | BT‐20J | 30326‐1 | 2.75" long | 0.710" ID | 0.736" OD | 0.013" wall | Blue
1 | ENGINE HOLDER | EH‐2 | 35021 | 2.8" long | .100" wide | .025" thick | 18/24mm | Thumb Saver
1 | ENGINE BLOCK | EB‐20‐2 | 30162‐2 | .69" OD | .542" ID | 0.19" long | BT‐5 in BT‐20 | Green
1 | RETAINER RING | HR‐20 | 030170‐3 | 0.5" long | 0.76" OD | 0.74" ID | 0.01" wall | Black
1 | CENTERING RING | AR‐201090 | 030151‐2 | 0.25" long | 0.737" ID | 1.043" OD | 0.153" wall | Green
1 | LAUNCH LUG | LL‐2C | 38180 | 5/32" ID | 1/8" rod | 5" long | | Mylar
1 | DIE‐CARD | SP‐2114 | 32431 | 1.5" wide | 4.25" long | 0.05" thick | with fin guide | Scan
1 | DIE‐CUT BALSA | KB‐2114 | 32812 | 3" wide | 9" long | 3/32" thick | | Scan
1 | TAPE RINGS | TD‐3F | 38407 | 1/2" dia. | Vinyl | Self‐Stick | W/Center Hole | Set of 6
1 | PARACHUTE | PK‐12A | 35820 | 12" dia. | 12" x 6 Shrouds | LDPE plastic | Org/Wht | Damon Logo
1 | *ELASTIC SHOCK CORD | SC‐1 | 38374 | 18" long | 1/8" wide | | | Rubber
1 | SHROUD LINE | SLT‐72 | 38237 | 72" | .020" diameter | Twisted cotton | 3 x 24" shrouds |
1 | DECAL SHEET | KD‐2114 | 37153 | 3.5" wide | 7" long | Blu, Yel | Selfstick | Scan
* plans call out Elastic but kit contains rubber.