PARTS LIST KIT N0. 0818 ‐ Rogue	
Quantity	

Description	

Type	
Number	

Details1	

Details2	

Details3	

Details4	

Comment	
1	BALSA NOSE CONE	BNC‐20R	70240	2.75" long	.736" dia.	.375" shoulder			
1	PAPER BODY TUBE	BT‐20B	30320	8.65" long	0.710" ID	0.736" OD	0.013" wall	Glassine	
1	PAPER BODY TUBE	BT‐5BJ	30304	2" long	0.515" ID	0.541" OD	0.013" wall	Glassine	
2	CENTERING RINGS	AR‐520	30162	.69" OD	.542" ID	0.25" long	Set of 2	Green	
1	ENGINE HOLDER	EH‐3	35026	1.8" long	.125" wide	.025" thick	13mm	Mini	
1	LAUNCH LUG	LL‐2A	38175	5/32" ID	1/8" rod	1.25" long		Mylar	
1	Die‐Cut Fin	BF‐0818	32272	3" wide	4" long	1/16" thick		Scan	
1	Decal	*KD‐0818	37318	2.5" wide	4.75" long	Blk, Wht	Waterslide	Scan	
1	Shock Cord	SC‐1	85730	18" long	1/8" wide			Rubber	
1	Parachute	PK‐10A	85562	10" dia.	12" x 6 Shrouds	LDPE plastic	Red/Wht	Damon Logo	
1	Tape Disc	TD‐3F	38406	1/2" dia.	Paper	Self‐Stick	WO/Center Hole	Set of 6	
1	Shroud Line	SLT‐72	38237	72"	.020" diameter	Twisted cotton	3 x 24" shrouds		
1	Screw Eye (Small)	SE‐2A	38252	3/4" long					
1	Dummy Engine Casing ‐ Mini	EC‐8	35014	0.5" OD	1.75" long	Empty Casing			
1	Display Stand	N/A	9014	3.5" wide	3.5" long	110 lb. Card	Blk/Wht	Scan	
1	Shock Cord Mount	N/A	N/A	On Instructions	Page 4	Paper	est0818d.png	Scan	
1	Marking Guide	N/A	82260A	On Instructions	Page 4	Paper	est0818d.png	Scan	
* Later versions had a different decal. The layout changed and the '3's were yellow instead of white.