PARTS LIST KIT N0. 1908 ‐ Scrambler 2	
Quantity	

Description	

Type	
Number	

Details1	

Details2	

Details3	

Details4	

Comment	
1	PAPER BODY TUBE	BT‐50J	30362	2.75" long	0.950" ID	0.976" OD	0.013" wall	Glassine	
1	ENGINE HOLDER	EH‐2	35025	2.8" long	.100" wide	.025" thick		Reg. & D	
2	CENTERING RINGS	AR‐5055	30166	.977" ID	1.27" OD	0.25" long			
1	CENTERING RINGS	AR‐2050	30164	0.25" long	0.737" ID	0.949" OD	0.106" wall	Green	
1	Body Marking Guide	SP‐1908	83639	3.5" wide	5" long	Heavy Cardstock		Scan	
1	PAPER BODY TUBE	BT‐55C	30383	14" long	1.283" ID	1.325" OD	0.021" wall	Glassine	
1	Shock Cord	SC‐1	85730	18" long	1/8" wide			Rubber	
1	BALSA FIN STOCK	*BFS‐30	32108	3" wide	9" long	3/32" thick	0.09375	Scan	
1	LAUNCH LUG	LL‐12	38166	5/32" ID	1/8" rod	2" long		Mylar	
1	PLASTIC NOSE CONE	*PNC‐60NA	72057	4.75" long	1.627" dia.	.75" shoulder	With TA‐5560 attached	Blow molded	
1	PAPER BODY TUBE	BT‐60R	30418	5" long	1.595" ID	1.637" OD	0.021" wall		
1	Parachute	PK‐12A	85564	12" hexagon	1.25 mil thick	LDPE plastic	Org/Wht		
1	Shroud Line	SLT‐72	38237	72"	.020" diameter	Twisted cotton			
2	Tape Disc	TD‐3F	38406	1/2" dia.	Paper	Self‐Stick		Set of 6	
1	Parachute	PK‐18A	85566	18" dia.	18" x 6 Shrouds	LDPE plastic	Org/Wht		
1	Shroud Line	SLT‐108	38239	108"	.020" diameter	Twisted cotton			
1	Decal Sheet	KD‐1908	37223	3" wide	9" long	Red/Wht/Blk	Waterslide	Scan	
1	Shock Cord	SC‐2	85736	18" long	1/4" wide			Rubber	
* Die‐Cut Balsa Sheet BF‐1908 Part #32608	
* Same used for Loadstar II #3227