Title: est1350_parts.xlsx
Author: JimZ

PARTS LIST KIT N0. 1350 ‐ Black Hole Space Probe
Quantity | Description | Type | Number | Details1 | Details2 | Details3 | Details4 | Comment
1 | PAPER BODY TUBE | BT‐20J | 30326 | 2.75" long | 0.710" ID | 0.736" OD | 0.013" wall | Glassine
1 | ENGINE HOLDER | EH‐2 | 35025 | 2.8" long | .100" wide | .025" thick | | Reg. & D
1 | MYLAR RETAINER RING | HR‐20 | 30168 | 0.3" long | 0.74" ID | 0.76" OD | 0.01" wall | BT‐20
1 | SPLIT ADAPTER RING | AR‐2050S | 80425 | 1/4" long | .737" ID | .949" OD | 0.106" wall | Green
1 | CENTERING RINGS | AR‐2050 | 30164 | 0.25" long | 0.737" ID | 0.949" OD | 0.106" wall | Green
1 | Shock Cord Mount | SCM‐50 | 84444 | 1.5" wide | 3" long | Heavy paper | For BT‐50 and larger | Scan
1 | Shock Cord | SC‐1 | 85730 | 18" long | 1/8" wide | | | Rubber
1 | PAPER BODY TUBE | BT‐50 | 30352 | 18" long | 0.950" ID | 0.976" OD | 0.013" wall | Glassine
1 | Pattern Sheet | SP‐1350 | 84233 | 5" wide | 9.5" long | Cardstock | | Scan
1 | BALSA WOOD STRIP | BWS‐40 | 85923 | 1/8" square | 12" long | | |
1 | Die‐Cut Card | TA‐1350 | 32950 | 0.98" ID | 1.275" OD | 0.02" thick | 12 rings | Scan
1 | BALSA FIN STOCK | *BFS‐30L | 3170 | 3" wide | 12" long | 3/32" thick | 0.09375 | Scan
3 | WOOD DOWEL | WD‐1S | 85904 | 1/8" dia. | 9" long | | | Wood
9 | LAUNCH LUG | LL‐2AM | 38176 | 5/32" ID | 1/8" rod | 3/8" long | | Mylar
1 | PLASTIC NOSE CONE | PNC‐50BB | 71027 | 5.7" long | .974" dia. | 0.5" shoulder | with attached nozzle | Blow Molded
1 | LAUNCH LUG | LL‐2B | 38178 | 5/32" ID | 1/8" rod | 2‐3/8" long | | Mylar
1 | Parachute | PK‐12A | 85564 | 12" hexagon | 1.25 mil thick | LDPE plastic | Org/Wht |
1 | Shroud Line | SLT‐72 | 38237 | 72" | .020" diameter | Twisted cotton | |
1 | Tape Disc | TD‐3F | 38406 | 1/2" dia. | Paper | Self‐Stick | | Set of 6
1 | Decal | KD‐1350 | 37590 | 4" wide | 6" long | Blk | Waterslide | Scan
*Die‐Cut Balsa Sheet (type BF‐1426) #32380

*Kit #1426 is the Black Hole Starter Kit . This set came with 3 engines, Solar igniters, Recovery Wadding, and the 6V Lantern Battery launch
pad.